## Diff of /osaf/services/saf/smfsv/schema/SAI-AIS-SMF-ETF-A.01.02_OpenSAF.xsd [6f40f2] .. [e07b4b] Maximize Restore

### Switch to side-by-side view

    --- a/osaf/services/saf/smfsv/schema/SAI-AIS-SMF-ETF-A.01.02_OpenSAF.xsd
    +++ b/osaf/services/saf/smfsv/schema/SAI-AIS-SMF-ETF-A.01.02_OpenSAF.xsd
    @@ -1,4 +1,4 @@
    -ďťż<?xml version="1.0" encoding="UTF-8"?>
    +<?xml version="1.0" encoding="UTF-8"?>
     <!-- edited with XMLSpy v2006 sp1 U (http://www.altova.com) by Maria Toeroe (Ericsson Canada/Open Systems Research) -->
     <xs:schema xmlns:xs="http://www.w3.org/2001/XMLSchema" elementFormDefault="qualified" attributeFormDefault="unqualified">
     	<!--
    @@ -20,6 +20,8 @@
        Note: This is a modified schema.
        ================================
        The following modifications have been made:
    +   Thu May 22 07:25:22 2014, Ingvar Bergstrom <ingvar.bergstrom@ericsson.com>
    +       smfsv: Comments in ETF schema for SaTimeT unified, all specifies nanoseconds [#925]
        Wed Aug 20 10:01:00 2013, Ingvar Bergstrom <ingvar.bergstrom@ericsson.com>
            smfsv: ETF and Campaign schemas are not matching each other (#460)
             -The component command arguments cardinality is changed from "single mandatory" to "0..*", i.e coluld be zero to infinite
    @@ -571,12 +573,12 @@
     				</xs:annotation>
     				<xs:element name="period" type="BoundedTimeT" minOccurs="0">
     					<xs:annotation>
    -						<xs:documentation>A healthcheck is run every "period" milliseconds. This attribue needs to be specified if there is any limitation on the frequency of healthchecks</xs:documentation>
    +						<xs:documentation>A healthcheck is run every "period" nanoseconds. This attribue needs to be specified if there is any limitation on the frequency of healthchecks</xs:documentation>
     					</xs:annotation>
     				</xs:element>
     				<xs:element name="maxDuration" type="BoundedTimeT" minOccurs="0">
     					<xs:annotation>
    -						<xs:documentation>Time in milliseconds during which the AMF expects the response to a healthcheck</xs:documentation>
    +						<xs:documentation>Time in nanoseconds during which the AMF expects the response to a healthcheck</xs:documentation>
     					</xs:annotation>
     				</xs:element>
     			</xs:sequence>
    @@ -665,7 +667,7 @@
     			<xs:element name="terminateCallbackTimeOut" type="BoundedTimeT" minOccurs="0">
     				<xs:annotation>
     					<xs:documentation>Time in nano-seconds in which AMF expects an SaAmfResponse call from the component after a preceding callback to terminate the component.
    -If a component has not responded within terminateCallbackTimeOut milliseconds it will be shut down by executing the termination command.</xs:documentation>
    +If a component has not responded within terminateCallbackTimeOut nanoseconds it will be shut down by executing the termination command.</xs:documentation>
     				</xs:annotation>
     			</xs:element>
     			<xs:element name="quiescingCompleteTimeout" type="BoundedTimeT" minOccurs="0">